

5-pin connector near STM32 chip.

Pin 1 has a rectangular contact area.

|  |  |  |
| --- | --- | --- |
| Standard ST-LINK/V2 20-pin connector |  | 5-pin connector |
| 1 | Vcc +3,3 Volts | 1 |
| 7 | SWDIO | 2 |
| 9 | SWCLK | 3 |
| 10 | GND | 4 |
| 15 | NRST | 5 |